IRremoteESP8266

Public Attributes | List of all members
HaierProtocol Union Reference

Native representation of a Haier HSU07-HEA03 A/C message. More...

`#include <ir_Haier.h>`

## Public Attributes
uint8_t | remote_state [kHaierACStateLength]
| < The state in native IR code form More...
struct {
uint8_t Prefix
uint8_t Command:4
uint8_t Temp:4
uint8_t CurrHours:5
uint8_t unknown:1
uint8_t SwingV:2
uint8_t CurrMins:6
uint8_t OffTimer:1
uint8_t OnTimer:1
uint8_t OffHours:5
uint8_t Health:1
uint8_t __pad0__:0
uint8_t OffMins:6
uint8_t Fan:2
uint8_t OnHours:5
uint8_t Mode:3
uint8_t OnMins:6
uint8_t Sleep:1
uint8_t __pad1__:0
uint8_t Sum
}; |

## Detailed Description

Native representation of a Haier HSU07-HEA03 A/C message.

## Member Data Documentation

## ◆ @55

struct { ... }

## ◆ __pad0__

uint8_t HaierProtocol::__pad0__

## ◆ __pad1__

uint8_t HaierProtocol::__pad1__

## ◆ Command

uint8_t HaierProtocol::Command

## ◆ CurrHours

uint8_t HaierProtocol::CurrHours

## ◆ CurrMins

uint8_t HaierProtocol::CurrMins

## ◆ Fan

uint8_t HaierProtocol::Fan

## ◆ Health

uint8_t HaierProtocol::Health

## ◆ Mode

uint8_t HaierProtocol::Mode

## ◆ OffHours

uint8_t HaierProtocol::OffHours

## ◆ OffMins

uint8_t HaierProtocol::OffMins

## ◆ OffTimer

uint8_t HaierProtocol::OffTimer

## ◆ OnHours

uint8_t HaierProtocol::OnHours

## ◆ OnMins

uint8_t HaierProtocol::OnMins

## ◆ OnTimer

uint8_t HaierProtocol::OnTimer

## ◆ Prefix

uint8_t HaierProtocol::Prefix

## ◆ remote_state

uint8_t HaierProtocol::remote_state[kHaierACStateLength]

< The state in native IR code form

## ◆ Sleep

uint8_t HaierProtocol::Sleep

## ◆ Sum

uint8_t HaierProtocol::Sum

## ◆ SwingV

uint8_t HaierProtocol::SwingV

## ◆ Temp

uint8_t HaierProtocol::Temp

## ◆ unknown

uint8_t HaierProtocol::unknown

The documentation for this union was generated from the following file:

- src/ir_Haier.h